**STEINEL Professional Bewegingsmelder**

**MD IR N270**

**COM1 - op de muur wit**

Dimensions (L x W x H): 87 x 82 x 98 mm; With motion detector: Ja; Manufacturer's Warranty: 5 jaar; Settings via: Bluetooth, Smartphone, Tablet; With remote control: Nee; Version: COM1 - op de muur wit; PU1, EAN: 4007841079819; Type: Bewegingsmelder; Application, place: Buiten, Binnen; Application, room: terras / balkon, rondom het huis, parkeergarage, tuin & oprit, Buiten, Binnen, entree; Colour: wit; Includes corner wall mount: Ja; Installation site: hoek, wand; Installation: Op de muur; IP-rating: IP54; Protection class: II; Ambient temperature: van -20 tot 40 °C; Materiaal: kunststof; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 2000 W; Switching output 1, number of LEDs / fluorescent lamps: 10 st; Power consumption: 0,3 W; Technology, sensors: passief infrarood, Lichtsensor; Mounting height: 1,80 – 6,00 m; Mounting height max.: 6,00 m; Optimum mounting height: 2 m; Detection angle: 270 °; Sneak-by guard: Ja; Capability of masking out individual segments: Ja; Electronic scalability: Ja; Mechanical scalability: Nee; Reach, radial: r = 2.7 m (17 m²); Reach, tangential: r = 12.5 m (368 m²); Cover material: afdekplaatjes; Functions: Lichtsensor, Bewegingssensor, Relaisuitgang, Gegevensbewaking; Twilight setting: 2 – 2000 lx; Time setting: 5 sec. – 60 min; Basic light level function: Nee; Main light adjustable: Nee; Twilight setting TEACH: Ja; Constant-lighting control: Nee; Interconnection: Ja; Interconnection via: Bluetooth; Reichweite Radial Eagle Eye max.: 6 m; Product category: Bewegingsmelder

**Fabrikant** Steinel

**art.nr.** 079819

**Bestelaanduiding** MD IR N270 COM1 - op de muur wit

Leveren, monteren en bedrijfsklaar instellen