STEINEL Professional Motion detector

MD IR N360
COM1 - surface white

Dimensions (L x W x H): 93 x 80 x 80 mm;Dimensions (Ø x H): 80 x 93 mm;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: Bluetooth, App;With remote control: No;Version: COM1 - surface white;PU1, EAN: 4007841080006;Type: Motion detectors;Application, place: Outdoors;Colour: white;Colour, RAL: 9010;Includes corner wall mount: No;Installation: Surface wiring;IP-rating: IP54;Ambient temperature: from -20 up to 40 °C;Material: Plastic;Mains power supply: 50 – 60 Hz;Fluorescent lamps, electronic ballast: 600 W;Fluorescent lamps, series-corrected: 1000 VA;Capacitive load in μF: 176 µF;Technology, sensors: passive infrared, Mixed light metering;Mounting height: 1,8 – 6,00 m;Mounting height max.: 6,00 m;Optimum mounting height: 2,5 m;Detection angle: 360 °;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: Yes;Mechanical scalability: No;Reach, radial: Ø 7 m (38 m²);Reach, tangential: Ø 26 m (531 m²);Switching zones: 1179 switching zones;Cover material: Cover clips;Twilight setting: 2 – 2000 lx;Time setting: 5 sec – 60 min;Twilight setting TEACH: Yes;Constant-lighting control: No;Interconnection: Yes;Interconnection via: Bluetooth Mesh;Reichweite Radial Eagle Eye max.: 6 m;Product category: Motion detector

Manufacturer Steinel
Prod. No. 080006
Ordering designation MD IR N360 COM1 - surface white

Deliver, install and set ready for operation
