**STEINEL Professional Composants du système**

**Relais REL5A-Bluetooth**

Dimensions (L x W x H): 20 x 46 x 45 mm; With motion detector: Non; Manufacturer's Warranty: 5 ans; Settings via: Connect Bluetooth Mesh, Application, Tablette, Smartphone; With remote control: Non; PU1, EAN: 4007841067335; Type: autre; Colour: blanc; Includes corner wall mount: Non; Installation: intégré, autre, Mur; IP-rating: IP20; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 1000 W; Switching output 1, number of LEDs / fluorescent lamps: 50 pcs.; LED lamps > 8 W: 300 W; Capacitive load in μF: 176 µF; With bus coupling: Non; Basic light level function: Non; Main light adjustable: Non; Twilight setting TEACH: Non; Constant-lighting control: Non; Interconnection: Oui; Interconnection via: Bluetooth Mesh; Product category: Composants du système

**Fabricant** Steinel

**Réf.** 067335

**Désignation commande** Relais REL5A-Bluetooth

Livrer, monter et régler pour être opérationnel