**STEINEL Professional Componenti del sistema**

**Relè REL5A-Bluetooth**

Dimensions (L x W x H): 20 x 46 x 45 mm; With motion detector: No; Manufacturer's Warranty: 5 anni; Settings via: Connect Bluetooth Mesh, App, Tablet, Smartphone; With remote control: No; PU1, EAN: 4007841067335; Type: altro; Colour: bianco; Includes corner wall mount: No; Installation: Incasso, altro, Parete; IP-rating: IP20; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 1000 W; Switching output 1, number of LEDs / fluorescent lamps: 50 pz; LED lamps > 8 W: 300 W; Capacitive load in μF: 176 µF; With bus coupling: No; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Sì; Interconnection via: Bluetooth Mesh; Product category: Componenti del sistema

**Produttore** Steinel

**Art. n.** 067335

**Denominazione ordine** Relè REL5A-Bluetooth

Consegnare, montare e impostare in modo che sia pronto alla messa in funzione