**STEINEL Professional Systeemonderdelen**

**Relais REL5A-Bluetooth**

Dimensions (L x W x H): 20 x 46 x 45 mm; With motion detector: Nee; Manufacturer's Warranty: 5 jaar; Settings via: Connect Bluetooth Mesh, App, Tablet, Smartphone; With remote control: Nee; PU1, EAN: 4007841067335; Type: overige; Colour: wit; Includes corner wall mount: Nee; Installation: In de muur, overige, Wand; IP-rating: IP20; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 1000 W; Switching output 1, number of LEDs / fluorescent lamps: 50 st; LED lamps > 8 W: 300 W; Capacitive load in μF: 176 µF; With bus coupling: Nee; Basic light level function: Nee; Main light adjustable: Nee; Twilight setting TEACH: Nee; Constant-lighting control: Nee; Interconnection: Ja; Interconnection via: Bluetooth Mesh; Product category: Systeemonderdelen

**Fabrikant** Steinel

**art.nr.** 067335

**Bestelaanduiding** Relais REL5A-Bluetooth

Leveren, monteren en bedrijfsklaar instellen