**STEINEL Professional System components**

**PC4 Bluetooth push-button coupler**

Dimensions (L x W x H): 15 x 43 x 50 mm; With motion detector: No; Manufacturer's Warranty: 5 years; Settings via: Connect Bluetooth Mesh, App, Tablet, Smartphone; With remote control: No; PU1, EAN: 4007841067342; Type: Other; Application, place: Indoors; Colour: white; Includes corner wall mount: No; Installation site: wall, ceiling; Installation: Installation, Other, Wall; IP-rating: IP20; Ambient temperature: from -20 up to 50 °C; Mains power supply: 220 – 240 V / 50 – 60 Hz; With bus coupling: No; Functions: 4 inputs for conventional switches, Semi-/fully automatic, Neighbouring group function, Push button configuration, Encrypted communication; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Interconnection via: Bluetooth Mesh; Product category: System components

**Manufacturer** Steinel

**Prod. No.** 067342

**Ordering designation** PC4 Bluetooth push-button coupler

Deliver, install and set ready for operation