**STEINEL Professional Composants du système**

**Coupleur à bouton-poussoir PC4-Bluetooth**

Dimensions (L x W x H): 15 x 43 x 50 mm; With motion detector: Non; Manufacturer's Warranty: 5 ans; Settings via: Connect Bluetooth Mesh, Application, Tablette, Smartphone; With remote control: Non; PU1, EAN: 4007841067342; Type: autre; Application, place: Intérieur; Colour: blanc; Includes corner wall mount: Non; Installation site: mur, plafond; Installation: intégré, autre, Mur; IP-rating: IP20; Ambient temperature: de -20 jusqu'à 50 °C; Mains power supply: 220 – 240 V / 50 – 60 Hz; With bus coupling: Non; Functions: 4 entrées pour boutons-poussoirs courants, Semi-automatique / Automatique, Fonction de groupe voisin, Configuration du bouton-poussoir, Communication cryptée; Basic light level function: Non; Main light adjustable: Non; Twilight setting TEACH: Non; Constant-lighting control: Non; Interconnection: Oui; Interconnection via: Bluetooth Mesh; Product category: Composants du système

**Fabricant** Steinel

**Réf.** 067342

**Désignation commande** Coupleur à bouton-poussoir PC4-Bluetooth

Livrer, monter et régler pour être opérationnel