**STEINEL Professional Systeemonderdelen**

**Drukknopschakelaar PC4-Bluetooth**

Dimensions (L x W x H): 15 x 43 x 50 mm; With motion detector: Nee; Manufacturer's Warranty: 5 jaar; Settings via: Connect Bluetooth Mesh, App, Tablet, Smartphone; With remote control: Nee; PU1, EAN: 4007841067342; Type: overige; Application, place: Binnen; Colour: wit; Includes corner wall mount: Nee; Installation site: wand, plafond; Installation: In de muur, overige, Wand; IP-rating: IP20; Ambient temperature: van -20 tot 50 °C; Mains power supply: 220 – 240 V / 50 – 60 Hz; With bus coupling: Nee; Functions: 4 ingangen voor gebruikelijke schakelaars, (Half-) automatisch, Buurgroepfunctie, Drukknop configuratie, Gecodeerde communicatie; Basic light level function: Nee; Main light adjustable: Nee; Twilight setting TEACH: Nee; Constant-lighting control: Nee; Interconnection: Ja; Interconnection via: Bluetooth Mesh; Product category: Systeemonderdelen

**Fabrikant** Steinel

**art.nr.** 067342

**Bestelaanduiding** Drukknopschakelaar PC4-Bluetooth

Leveren, monteren en bedrijfsklaar instellen