STEINEL Professional Presence detector

IR Quattro HD-2 24m
COM1 - surface black

Dimensions (L x W x H): 64 x 123 x 123 mm;Manufacturer's Warranty: 5 years;Settings via: Bluetooth Mesh, App, Potentiometers, Smartphone;With remote control: No;Version: COM1 - surface black;PU1, EAN: 4007841094515;Type: Presence detector;Application, place: Indoors;Application, room: lecture hall, classroom, open-plan office, high-bay warehouse, production facilities, conference room / meeting room, duty room, recreation room, changing room, reception / lobby, sports hall, multi-storey / underground car park, dining hall / staff restaurant, Indoors;Colour: black;Colour, RAL: 9005;Includes corner wall mount: No;Installation site: ceiling;Installation: Surface wiring, Ceiling;IP-rating: IP54;Ambient temperature: from -20 up to 50 °C;Material: Plastic;Mains power supply: 220 – 240 V / 50 – 60 Hz;Switching output 1, resistive: 2000 W;Switching output 1, number of LEDs / fluorescent lamps: 8 pcs.;Switching output 1, floating: No;Fluorescent lamps, electronic ballast: 1500 W;Fluorescent lamps, uncorrected: 1000 VA;Fluorescent lamps, series-corrected: 400 VA;Fluorescent lamps, parallel-corrected: 1000 VA;Switching output 1, low-voltage halogen lamps: 2000 VA;LED lamps < 2 W: 100 W;LED lamps > 2 W < 8 W: 300 W;LED lamps > 8 W: 600 W;Capacitive load in μF: 176 µF;Power consumption: 0,3 W;Technology, sensors: Mixed light metering, passive infrared;Voltage range (min): 220 V;Voltage range (max): 240 V;Mounting height: 2,50 – 10,00 m;Mounting height max.: 10,00 m;Optimum mounting height: 2,8 m;Detection angle: 360 °;Capability of masking out individual segments: Yes;Electronic scalability: Yes;Mechanical scalability: Yes;Reach, radial: 9 x 9 m (81 m²);Reach, tangential: 24 x 24 m (576 m²);Reach, presence: 9 x 9 m (81 m²);Functions: Group parameterisation, Semi-/fully automatic, Manual ON / ON-OFF, Neighbouring group function, Normal / test mode;Twilight setting: 2 – 2000 lx;Time setting: 5 sec – 60 min;Basic light level function: No;Main light adjustable: Yes;Twilight setting TEACH: Yes;Constant-lighting control: No;Interconnection: Yes;Interconnection via: Bluetooth Mesh;Product category: Presence detector

Manufacturer Steinel
Prod. No. 094515
Ordering designation IR Quattro HD-2 24m COM1 - surface black

Deliver, install and set ready for operation
