STEINEL Professional Motion detector


white

Dimensions (Ø x H): 78 x 89 mm;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: Potentiometers;With remote control: No;Version: white;PU1, EAN: 4007841034733;Type: Motion detectors;Application, place: Outdoors, Indoors;Application, room: corridor / aisle, changing room, function room / ancillary room, kitchenette, stairwell, WC / washroom, outdoors, front door, all round the building, terrace / balcony, Indoors;Colour: white;Colour, RAL: 9010;Includes corner wall mount: No;Installation site: ceiling;Installation: In-ceiling installation, Ceiling;IP-rating: IP54;Protection class: II;Ambient temperature: from -20 up to 40 °C;Material: Plastic;Mains power supply: 220 – 240 V / 50 – 60 Hz;Fluorescent lamps, electronic ballast: 350 W;Fluorescent lamps, uncorrected: 500 VA;Fluorescent lamps, series-corrected: 500 VA;Fluorescent lamps, parallel-corrected: 500 VA;Switching output 1, low-voltage halogen lamps: 1000 VA;LED lamps < 2 W: 100 W;LED lamps > 2 W < 8 W: 175 W;LED lamps > 8 W: 350 W;Capacitive load in μF: 132 µF;Technology, sensors: passive infrared, Mixed light metering;Mounting height: 2,2 – 4 m;Mounting height max.: 4,00 m;Optimum mounting height: 2,5 m;Detection angle: 360 °;Angle of aperture: 180 °;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: No;Mechanical scalability: No;Reach, radial: Ø 4 m (13 m²);Reach, tangential: Ø 8 m (50 m²);Switching zones: 304 switching zones;Cover material: shrouds;Twilight setting: 2 – 2000 lx;Time setting: 8 sec – 35 min;Basic light level function: No;Main light adjustable: No;Twilight setting TEACH: No;Constant-lighting control: No;Interconnection: Yes;Type of interconnection: Master/master;Interconnection via: Cable;Product category: Motion detector

Manufacturer Steinel
Prod. No. 034733
Ordering designation 

Deliver, install and set ready for operation
