STEINEL DIY Outdoor light without sensor

L 30
without motion detector

Dimensions (L x W x H): 108 x 122 x 261 mm;With lamp: No;Manufacturer's Warranty: 3 years;With remote control: No;Version: without motion detector;PU1, EAN: 4007841068882;Application, place: Outdoors;Application, room: garden, front door, courtyard & driveway, all round the building, terrace / balcony;Colour: Anthracite;includes sheet of self-adhesive numbers: No;Package content: 1;Installation site: wall;Impact resistance: IK07;IP-rating: IP44;Protection class: II;Ambient temperature: from -20 up to 40 °C;Housing material: Plastic;Cover material: Plastic, opal;Mains power supply: 220 – 240 V / 50 – 60 Hz;Output: 15 W;Base: E27;Interconnection: No;Product category: Outdoor light without sensor

Manufacturer Steinel
Prod. No. 068882
Ordering designation L 30 without motion detector

Deliver, install and set ready for operation
