STEINEL DIY Solar light

XSolar LH-N
Anthracite

Application, room: outdoors, front door, courtyard & driveway;Dimensions (L x W x H): 50 x 242 x 227 mm;Colour: Anthracite;Sensor Technology: Light sensor;Output: 0,03 W;Colour Rendering Index: 60-69;Colour temperature: 4000 K;With lamp: Yes, STEINEL LED system;LED life expectancy (max. °C): 50000 h;Lamp: LED cannot be replaced;Base: without;LED cooling system: Passive Thermo Control;With motion detector: No;Photo-cell controller: Yes;Twilight setting: 2 lx;Basic light level function time: all night;Soft light start: No;Manual override: No;Impact resistance: IK03;IP-rating: IP44;Protection class: III;Glow-wire test: 650°C - 30 s;Ambient temperature: from -20 up to 40 °C;Cover material: Plastic, opal;Housing material: Stainless steel;Manufacturer's Warranty: 3 years;PU1, EAN: 4007841035730

Manufacturer Steinel
Prod. No. 035730
Ordering designation XSolar LH-N Anthracite

Deliver, install and set ready for operation
