STEINEL DIY LED outdoor light without sensor

GL 65
without motion detector

With lamp: Yes, LED lamp;Manufacturer's Warranty: 3 years;With remote control: No;Version: without motion detector;PU1, EAN: 4007841069469;Application, place: Outdoors;Application, room: outdoors, garden, front door, courtyard & driveway, all round the building;Colour: Anthracite;includes sheet of self-adhesive numbers: No;Package content: 1;Installation site: Stand mounted;Impact resistance: IK03;IP-rating: IP44;Protection class: I;Ambient temperature: from -20 up to 40 °C;Housing material: Aluminium;Cover material: Glass opal;Mains power supply: 220 – 240 V / 50 – 60 Hz;Output: 8,5 W;Luminous flux total product: 575 lm;Measured luminos flux (360°): 575 lm;Total product efficiency: 68 lm/W;Colour temperature: 3000 K;Lamp: LED cannot be replaced;Service life LED L70B50 (25°): > 36000 h;LED cooling system: Passive Thermo Control;Soft light start: Yes;Interconnection: No;Colour Rendering Index CRI: = 80;Product category: LED outdoor light without sensor

Manufacturer Steinel
Prod. No. 069469
Ordering designation GL 65 without motion detector

Deliver, install and set ready for operation
