STEINEL DIY LED outdoor light without sensor

L 271 digi C
without motion detector, with Bluetooth

Dimensions (L x W x H): 65 x 116 x 235 mm;With lamp: Yes, STEINEL LED system;Manufacturer's Warranty: 3 years;With remote control: No;Version: without motion detector, with Bluetooth;PU1, EAN: 4007841068714;Application, place: Outdoors;Application, room: garden, front door, all round the building, terrace / balcony;Colour: Anthracite;includes sheet of self-adhesive numbers: No;Package content: 1;Installation site: wall;Impact resistance: IK03;IP-rating: IP44;Protection class: II;Ambient temperature: from -10 up to 40 °C;Housing material: Aluminium;Cover material: Plastic, opal;Mains power supply: 220 – 240 V / 50 – 60 Hz;Output: 6,6 W;Average rated life expectancy of power supply unit at 25°C: > 60000 h;Luminous flux total product: 566 lm;Measured luminos flux (360°): 566 lm;Total product efficiency: 85 lm/W;Colour temperature: 3000 K;Lamp: LED cannot be replaced;Continuous light: selectable;Interconnection: Yes;Interconnection via: Bluetooth Mesh;Colour Rendering Index CRI: = 82;Product category: LED outdoor light without sensor

Manufacturer Steinel
Prod. No. 068714
Ordering designation L 271 digi C without motion detector, with Bluetooth

Deliver, install and set ready for operation
