STEINEL DIY Outdoor light without sensor

L 810 C
Anthracite

Dimensions (L x W x H): 146 x 230 x 91 mm;With lamp: Yes, STEINEL LED system;Manufacturer's Warranty: 3 years;Settings via: App, Bluetooth;With remote control: No;Version: Anthracite;PU1, EAN: 4007841079307;Application, place: Outdoors;Application, room: garden, front door, courtyard & driveway, all round the building, terrace / balcony;Colour: Anthracite;includes sheet of self-adhesive numbers: No;Package content: 1;Installation site: wall;Impact resistance: IK03;IP-rating: IP44;Protection class: II;Ambient temperature: from -20 up to 40 °C;Housing material: Aluminium;Cover material: Plastic, opal;Mains power supply: 220 – 240 V / 50 – 60 Hz;Output: 9,8 W;Mounting height max.: 2,50 m;Transmitter power: < 1 mW;Luminous flux total product: 679 lm;Measured luminos flux (360°): 679 lm;Total product efficiency: 69 lm/W;Colour temperature: 3000 K;Lamp: LED cannot be replaced;Service life LED L70B50 (25°): > 60000 h;Base: without;LED cooling system: Active and Passive Thermo Control;Soft light start: Yes;Interconnection: Yes;Interconnection via: Bluetooth;Colour Rendering Index CRI: = 82;Optimum mounting height: 2 m;Product category: Outdoor light without sensor

Manufacturer Steinel
Prod. No. 079307
Ordering designation L 810 C Anthracite

Deliver, install and set ready for operation
