STEINEL DIY Outdoor light without sensor

L 930
without motion detector

Dimensions (L x W x H): 92 x 63 x 137 mm;With lamp: Yes, STEINEL LED system;With remote control: No;Version: without motion detector;PU1, EAN: 4007841078713;Application, place: Outdoors;Application, room: outdoors, front door, all round the building, terrace / balcony, garden;Colour: Anthracite;includes sheet of self-adhesive numbers: No;Package content: 1;Installation site: wall;Impact resistance: IK03;IP-rating: IP44;Protection class: I;Ambient temperature: from -20 up to 40 °C;Housing material: Aluminium;Cover material: Plastic, opal;Mains power supply: 220 – 240 V / 50 – 60 Hz;Output: 9,3 W;Luminous flux total product: 457 lm;Measured luminos flux (360°): 457 lm;Total product efficiency: 49 lm/W;Colour temperature: 3000 K;Colour variation LED: SDCM3;Lamp: LED cannot be replaced;Service life LED L70B50 (25°): > 60000 h;Base: without;LED cooling system: Passive Thermo Control;Soft light start: No;Interconnection: No;Colour Rendering Index CRI: = 82;Product category: Outdoor light without sensor

Manufacturer Steinel
Prod. No. 078713
Ordering designation L 930 without motion detector

Deliver, install and set ready for operation
