STEINEL DIY Sensor-switched LED outdoor light

L 940 SC
with motion detector & Bluetooth

Dimensions (L x W x H): 115 x 70 x 160 mm;With lamp: Yes, LED lamp;Manufacturer's Warranty: 3 years;Settings via: Bluetooth Mesh;With remote control: No;Version: with motion detector & Bluetooth;PU1, EAN: 4007841087739;Application, place: Outdoors;Application, room: outdoors, front door, all round the building, terrace / balcony;Colour: Anthracite;includes sheet of self-adhesive numbers: No;Package content: 1;Installation site: wall;IP-rating: IP44;Protection class: I;Ambient temperature: from -20 up to 40 °C;Housing material: Aluminium;Cover material: PC structured;Mains power supply: 220 – 240 V / 50 – 60 Hz;Output: 14,5 W;Mounting height max.: 4,00 m;Slave modeselectable: Yes;Sneak-by guard: No;Capability of masking out individual segments: No;Electronic scalability: No;Mechanical scalability: No;Reach, radial: r = 3 m (14 m²);Reach, tangential: r = 8.5 m (113 m²);Photo-cell controller: Yes;Luminous flux total product: 1240 lm;Colour temperature: 3000 K;Lamp: LED can be replaced;Service life LED L70B50 (25°): > 20000 h;Base: GU10;Soft light start: No;Functions: Motions sensor, Light sensor, Neighbouring group function, Push button configuration, Pushbutton / switch mode;Twilight setting: 2 – 1000 lx;Time setting: 5 sec – 60 min;Basic light level function: No;Main light adjustable: No;Twilight setting TEACH: Yes;Interconnection: Yes;Type of interconnection: Sensor/slave;Interconnection via: Bluetooth Mesh;Colour Rendering Index CRI: = 81;R9-Farbwiedergabeindex: -0,4;Optimum mounting height: 1,8 m;Detection angle: 180 °;Product category: Sensor-switched LED outdoor light

Manufacturer Steinel
Prod. No. 087739
Ordering designation L 940 SC with motion detector & Bluetooth

Deliver, install and set ready for operation
