STEINEL DIY Sensor-switched LED floodlight

LS 300 S
white

Dimensions (L x W x H): 186 x 213 x 241 mm;With lamp: Yes, STEINEL LED system;With motion detector: Yes;Manufacturer's Warranty: 3 years;Settings via: Potentiometers;Version: white;PU1, EAN: 4007841067588;Application, place: Outdoors;Application, room: outdoors, all round the building, courtyard & driveway;Colour: white;Includes corner wall mount: No;Installation site: wall;Installation: Wall, Surface wiring;Impact resistance: IK03;IP-rating: IP44;Protection class: I;Ambient temperature: from -10 up to 30 °C;Housing material: Aluminium;Cover material: Glass transparent;Mains power supply: 220 – 240 V / 50 – 60 Hz;Power consumption: 30,4 W;Mounting height max.: 4,00 m;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: No;Mechanical scalability: No;Reach, radial: r = 3.5 m (26 m²);Reach, tangential: r = 12 m (302 m²);Photo-cell controller: Yes;Luminous flux total product: 2704 lm;Measured luminos flux (360°): 2962 lm;Total product efficiency: 92 lm/W;Colour temperature: 4000 K;Colour variation LED: SDCM3;Lamp: LED cannot be replaced;LED life expectancy (max. °C): 50000 h;Service life LED L70B50 (25°): > 36000 h;Drop in luminous flux in accordance with LM80: L70B10;LED cooling system: Passive Thermo Control;Soft light start: No;Twilight setting: 2 – 1000 lx;Time setting: 10 sec – 15 min;Basic light level function: No;Interconnection: No;Output: 29,5 W;Colour Rendering Index CRI: = 80;Optimum mounting height: 2 m;Detection angle: 240 °;Product category: Sensor-switched LED floodlight;Energy efficiency class of light source: F

Manufacturer Steinel
Prod. No. 067588
Ordering designation LS 300 S white

Deliver, install and set ready for operation
