STEINEL Professional Presence detector

LuxMaster True Presence
DALI-2 APC - surface

Dimensions (L x W x H): 45 x 123 x 123 mm;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: Bluetooth Mesh;With remote control: No;Version: DALI-2 APC - surface;PU1, EAN: 4007841085582;Type: Presence detector;Application, place: Indoors;Application, room: classroom, lecture hall, one-person office, open-plan office, high-bay warehouse, production facilities, conference room / meeting room, hotel room, care room, duty room, recreation room, dining hall / staff restaurant, changing room, kitchenette, sports hall, reception / lobby, WC / washroom, warehouse, Indoors;Colour: white;Colour, RAL: 9003;Includes corner wall mount: No;Installation site: ceiling;Installation: Surface wiring, Ceiling;IP-rating: IP54;Ambient temperature: from -20 up to 50 °C;Material: Plastic;Mains power supply: 220 – 240 V / 50 – 60 Hz;Number of Dali users: 64;Control output, Dali: Broadcast 64 electronic ballasts / Addressable;Technology, sensors: High frequency, Mixed light metering;Mounting height: 2,00 – 12,00 m;Mounting height max.: 12,00 m;Optimum mounting height: 2,8 m;Montagehöhe max. True Presence Erfassung: 4,00 m;HF-system: 7,2 GHz;Detection: also through glass, wood and stud walls;Detection angle: 360 °;Angle of aperture: 160 °;Sneak-by guard: Yes;Capability of masking out individual segments: No;Electronic scalability: Yes;Mechanical scalability: No;Reach, radial: Ø 15 m (177 m²);Reach, tangential: Ø 15 m (177 m²);Reach, presence: Ø 15 m (177 m²);True Presence reach: Ø 9 m (64 m²);Transmitter power: < 1 mW;Functions: Selecting programmed lighting scenarios, Semi-/fully automatic, Constant-lighting control ON-OFF, Lighting scenario, Manual ON / ON-OFF, Neighbouring group function, Normal / test mode, TouchDIM function;Twilight setting: 2 – 2000 lx;Time setting: 20 sec – 60 min;Basic light level function: Yes;Basic light level function time: 1-60 min, all night;Main light adjustable: 10 - 100 %;Twilight setting TEACH: Yes;Constant-lighting control: Yes;Interconnection: Yes;Type of interconnection: Master/master, Master/slave;Interconnection via: Bluetooth Mesh;Product category: Presence detector

Manufacturer Steinel
Prod. No. 085582
Ordering designation LuxMaster True Presence DALI-2 APC - surface

Deliver, install and set ready for operation
