STEINEL Professional Motion detector

sensIQ
KNX - black V3.1

Dimensions (L x W x H): 172 x 113 x 144 mm;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: ETS software, Remote control, Bus, Smart Remote;With remote control: Yes;Version: KNX - black;PU1, EAN: 4007841059552;Type: Motion detectors;Application, place: Outdoors, Indoors;Application, room: multi-storey / underground car park, outdoors, warehouse, front door, all round the building, courtyard & driveway, Indoors;Colour: black;Colour, RAL: 9005;Includes corner wall mount: Yes;Installation site: wall, ceiling, corner;Installation: Surface wiring, Wall, Ceiling, corner;IP-rating: IP54;Ambient temperature: from -20 up to 50 °C;Material: Plastic;With bus coupling: Yes;Technology, sensors: passive infrared;Mounting height: 2 – 5 m;Mounting height max.: 5,00 m;Optimum mounting height: 2 m;Detection angle: 300 °;Angle of aperture: 180 °;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: Yes;Mechanical scalability: Yes;Reach, radial: r = 4 m (42 m²);Reach, tangential: r = 20 m (1047 m²);Switching zones: 1360 switching zones;Twilight setting: 2 – 1000 lx;Time setting: 60 sec – 255 min;Basic light level function: Yes;Basic light level function time: 1-255 min;Main light adjustable: 0 - 100 %;Twilight setting TEACH: Yes;Constant-lighting control: Yes;KNX functions: Light output 2x, Presence output, Light level, Constant-lighting control, Basic light level function, Photo-cell controller, Close range, Individual pyro evaluation, Logic gate;Interconnection: Yes;Type of interconnection: Master/master, Master/slave;Interconnection via: KNX bus;Rated current: 10 mA;KNX Medium: TP 256;KNX Secure: No;Product category: Motion detector

Manufacturer Steinel
Prod. No. 059552
Ordering designation sensIQ KNX - black

Deliver, install and set ready for operation
