STEINEL Professional Multisensor

Multisensor EO
IP - surface black

Dimensions (L x W x H): 123 x 123 x 44 mm;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: Bluetooth Mesh;With remote control: No;Version: IP - surface black;PU1, EAN: 4007841091194;Application, place: Indoors;Colour: black;Includes corner wall mount: No;Installation site: ceiling;Installation: Surface wiring;IP-rating: IP20;Mains power supply: 44 – 57 V;Power supply, detail: Passive PoE SELV, standard PoE (IEEE 802.3 af);Technology, sensors: CO2, Air pressure, Air humidity, Temperature, VOC;Mounting height: 2,5 – 3,5 m;Mounting height max.: 3,50 m;Optimum mounting height: 2,8 m;Detection angle: 360 °;Capability of masking out individual segments: Yes;Electronic scalability: Yes;Mechanical scalability: No;Twilight setting TEACH: No;Interconnection: Yes;Interconnection via: Bluetooth Mesh;Product category: Multisensor;Erfassungsfläche bei Montagehöhe: 2.5 m: 6.6 x 4.2 m (28 m²), <br/>3.0 m: 5.0 x 8.0 m (40 m²), <br/>3.5 m: 5.9 x 9.3 m (55 m²);Anzahl von Erfassungszonen: 10

Manufacturer Steinel
Prod. No. 091194
Ordering designation Multisensor EO IP - surface black

Deliver, install and set ready for operation
