STEINEL Professional Photoelectric lighting controller

TS basic
Anthracite

Dimensions (L x W x H): 38 x 95 x 95 mm;With motion detector: No;Manufacturer's Warranty: 5 years;Settings via: Potentiometers;With remote control: No;Version: Anthracite;PU1, EAN: 4007841099688;Type: Photo-cell controller;Application, place: Outdoors;Application, room: outdoors, front door, courtyard & driveway, Indoors, all round the building, terrace / balcony;Colour: Anthracite;Installation site: wall;Installation: Surface wiring, Wall;IP-rating: IP54;Ambient temperature: from -20 up to 40 °C;Mains power supply: 220 – 240 V / 50 – 60 Hz;LED lamps > 2 W < 8 W: 250 W;LED lamps > 8 W: 250 W;Technology, sensors: Mixed light metering;Voltage range (min): 220 V;Voltage range (max): 240 V;Twilight setting: 1 – 75 lx;Basic light level function: No;Main light adjustable: No;Constant-lighting control: No;Interconnection: Yes;Interconnection via: Cable;Product category: Photoelectric lighting controller

Manufacturer Steinel
Prod. No. 099688
Ordering designation TS basic Anthracite

Deliver, install and set ready for operation
