STEINEL Professional Motion detector

MD IR 2180N
COM1 - white

With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: Potentiometers;With remote control: No;Version: COM1 - white;PU1, EAN: 4007841095895;Type: Motion detectors;Includes corner wall mount: No;Installation: Surface wiring, Wall;IP-rating: IP54;Ambient temperature: from -20 up to 40 °C;Material: Plastic;Mains power supply: 220 – 240 V / 50 – 60 Hz;Switching output 1, resistive: 1000 W;Switching output 1, floating: No;LED lamps > 2 W < 8 W: 350 W;LED lamps > 8 W: 350 W;Power consumption: 0,11 W;Technology, sensors: passive infrared, Mixed light metering;Voltage range (min): 220 V;Voltage range (max): 240 V;Mounting height: 2 – 4 m;Mounting height max.: 4,00 m;Optimum mounting height: 2 m;Detection angle: 180 °;Angle of aperture: 90 °;Sneak-by guard: No;Capability of masking out individual segments: Yes;Electronic scalability: No;Reach, radial: r = 5 m (39 m²);Reach, tangential: r = 17 m (454 m²);Cover material: sticker;Twilight setting: 2 – 1000 lx;Time setting: 8 sec – 35 min;Basic light level function: No;Main light adjustable: No;Twilight setting TEACH: No;Constant-lighting control: No;Product category: Motion detector

Manufacturer Steinel
Prod. No. 095895
Ordering designation MD IR 2180N COM1 - white

Deliver, install and set ready for operation
