STEINEL DIY Motion detector

IS 180 Flex Connect
black

Dimensions (L x W x H): 117 x 82 x 87 mm;With motion detector: Yes;Manufacturer's Warranty: 3 years;Settings via: Bluetooth Mesh;With remote control: No;Version: black;PU1, EAN: 4007841068790;Type: Motion detectors;Application, place: Outdoors, Indoors;Application, room: outdoors, stairwell, all round the building, courtyard & driveway;Colour: black;Includes corner wall mount: No;Installation site: wall;Package content: 1;IP-rating: IP54;Ambient temperature: from -20 up to 40 °C;Material: Plastic;Mains power supply: 220 – 240 V / 50 – 60 Hz;Switching output 1, number of LEDs / fluorescent lamps: 50 pcs.;Fluorescent lamps, electronic ballast: 250 W;Capacitive load in μF: 132 µF;Technology, sensors: passive infrared;Voltage range (min): 220 V;Voltage range (max): 240 V;Mounting height: 1,80 – 4,00 m;Mounting height max.: 4,00 m;Optimum mounting height: 2 m;Cover material: sticker;Functions: Motions sensor, Light sensor, Relay output, Semi-/fully automatic, Normal / test mode, Push button configuration;Twilight setting: 2 – 2000 lx;Time setting: 5 sec – 60 min;Basic light level function: No;Main light adjustable: No;Constant-lighting control: No;Interconnection: Yes;Interconnection via: Bluetooth Mesh, Cable;Product category: Motion detector

Manufacturer Steinel
Prod. No. 068790
Ordering designation IS 180 Flex Connect black

Deliver, install and set ready for operation
