STEINEL DIY Motion detector

IS 180 Flex
black

Dimensions (L x W x H): 117 x 82 x 87 mm;With motion detector: Yes;Manufacturer's Warranty: 3 years;Settings via: Potentiometers;With remote control: No;Version: black;PU1, EAN: 4007841068769;Type: Motion detectors;Application, place: Outdoors, Indoors;Application, room: outdoors, stairwell, all round the building, courtyard & driveway;Colour: black;Includes corner wall mount: No;Installation site: wall;Package content: 1;IP-rating: IP54;Ambient temperature: from -20 up to 40 °C;Material: Plastic;Mains power supply: 220 – 240 V / 50 – 60 Hz;Switching output 1, number of LEDs / fluorescent lamps: 50 pcs.;Fluorescent lamps, electronic ballast: 250 W;Capacitive load in μF: 132 µF;Technology, sensors: passive infrared;Voltage range (min): 220 V;Voltage range (max): 240 V;Mounting height: 1,80 – 4,00 m;Mounting height max.: 4,00 m;Optimum mounting height: 2 m;Sneak-by guard: No;Capability of masking out individual segments: Yes;Electronic scalability: No;Mechanical scalability: Yes;Reach, radial: r = 5 m (39 m²);Reach, tangential: r = 17 m (454 m²);Cover material: sticker;Functions: Motions sensor, Light sensor, Relay output;Twilight setting: 2 – 1000 lx;Time setting: 8 sec – 35 min;Basic light level function: No;Main light adjustable: No;Twilight setting TEACH: No;Constant-lighting control: No;Interconnection: Yes;Interconnection via: Cable;Product category: Motion detector

Manufacturer Steinel
Prod. No. 068769
Ordering designation IS 180 Flex black

Deliver, install and set ready for operation
