STEINEL Professional E27 Sensor-switched outdoor light

L 400 S
black

Dimensions (L x W x H): 250 x 215 x 336 mm;With lamp: No;Manufacturer's Warranty: 5 years;Settings via: Potentiometers;With remote control: No;Version: black;PU1, EAN: 4007841611019;Application, place: Outdoors;Application, room: outdoors, front door, all round the building, terrace / balcony, courtyard & driveway;Colour: black;Package content: 1;Installation site: wall;Impact resistance: IK03;IP-rating: IP44;Protection class: II;Ambient temperature: from -20 up to 40 °C;Housing material: Plastic;Cover material: Glass transparent;Mains power supply: 220 – 240 V / 50 – 60 Hz;Output: 60 W;Power consumption: 0,8 W;Mounting height max.: 6,00 m;Slave modeselectable: No;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: No;Mechanical scalability: No;Reach, radial: r = 3 m (19 m²);Reach, tangential: r = 12 m (302 m²);Photo-cell controller: Yes;Cover material: shrouds;Lamp: All-purpose lamp;Base: E27;Soft light start: Yes;Continuous light: selectable, 4h;Twilight setting: 2 – 2000 lx;Time setting: 5 sec – 15 min;Basic light level function: Yes;Interconnection: No;Basic light level function in per cent: 0 – 50 %;Basic light level function percentage, from: 0 %;Basic light level function percentage, up to: 50 %;Optimum mounting height: 2 m;Detection angle: 240 °;Product category: E27 Sensor-switched outdoor light

Manufacturer Steinel
Prod. No. 611019
Ordering designation L 400 S black

Deliver, install and set ready for operation
