**STEINEL Professional Motion detector**

**HF 3360**

**DALI-2 Input Device - surface, rd.**

Dimensions (Ø x H): 126 x 52 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bus; With remote control: No; Version: DALI-2 Input Device - surface, rd.; PU1, EAN: 4007841057329; Type: Motion detectors; Application, place: Indoors; Application, room: function room / ancillary room, stairwell, WC / washroom, multi-storey / underground car park, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: wall, ceiling, corner; Installation: Surface wiring, Wall, Ceiling, corner; IP-rating: IP54; Ambient temperature: -20 – 50 °C; Material: Plastic; Mains power supply: 12 – 22,5 V; Power consumption: 0,5 W; Power supply, detail: DALI bus; Number of Dali users: 5; Steuerausgang, Dali: Addressable/slave; With bus coupling: Yes; Technology, sensors: High frequency, Light sensor; Mounting height: 2,00 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 8 m (50 m²); Reach, tangential: Ø 8 m (50 m²); Transmitter power: < 1 mW; Twilight setting: 2 – 1000 lx; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: DALI bus; Max. Current consumption according to IEC 62386-101: 24 mA; Typical current consumption at 16V input voltage: 8 mA; Max. Current consumption at 10V input voltage in regular operation: 12 mA

**Manufacturer** Steinel

**Prod. No.** 057329

**Ordering designation** HF 3360 DALI-2 Input Device - surface, rd.

Deliver, install and set ready for operation