STEINEL Professional Motion detector

IS 2180 ECO
Anthracite

Dimensions (L x W x H): 55 x 78 x 120 mm;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: Potentiometers;With remote control: No;Version: Anthracite;PU1, EAN: 4007841064907;Type: Motion detectors;Application, place: Outdoors;Application, room: outdoors, front door, all round the building, terrace / balcony, courtyard & driveway;Colour: Anthracite;Colour, RAL: 7016;Includes corner wall mount: No;Installation site: wall, corner;Package content: 1;Installation: Surface wiring, Wall, corner;IP-rating: IP54;Ambient temperature: from -20 up to 50 °C;Material: Plastic;Mains power supply: 230 V / 50 Hz;Switching output 1, resistive: 2000 W;Switching output 1, floating: No;Fluorescent lamps, electronic ballast: 350 W;Fluorescent lamps, uncorrected: 500 VA;Fluorescent lamps, series-corrected: 900 VA;Fluorescent lamps, parallel-corrected: 500 VA;Switching output 1, low-voltage halogen lamps: 1000 VA;LED lamps < 2 W: 100 W;LED lamps > 2 W < 8 W: 175 W;LED lamps > 8 W: 350 W;Capacitive load in μF: 132 µF;Power consumption: 0,5 W;Technology, sensors: passive infrared, Mixed light metering;Voltage range (min): 230 V;Voltage range (max): 230 V;Mounting height: 1,8 – 4 m;Mounting height max.: 4,00 m;Optimum mounting height: 2 m;Detection angle: 180 °;Angle of aperture: 90 °;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: No;Mechanical scalability: No;Reach, radial: r = 1.5 m (4 m²) / r = 3 m (14 m²);Reach, tangential: r = 5 m (39 m²) / r = 12 m (226 m²);Switching zones: 508 switching zones;Cover material: shrouds;Twilight setting: 2 – 2000 lx;Time setting: 10 sec – 15 min;Basic light level function: No;Main light adjustable: No;Twilight setting TEACH: No;Constant-lighting control: No;Interconnection: Yes;Type of interconnection: Master/master;Interconnection via: Cable;Product category: Motion detector

Manufacturer Steinel
Prod. No. 064907
Ordering designation IS 2180 ECO Anthracite

Deliver, install and set ready for operation
