**STEINEL Professional Sensore di movimento**

**IS 2180-2**

**antracite**

Dimensions (L x W x H): 55 x 78 x 120 mm; With motion detector: Sì; Manufacturer's Warranty: 5 anni; Settings via: Potenziometri; With remote control: No; Version: antracite; PU1, EAN: 4007841057664; Type: Rilevatori di movimento; Application, place: Esterno, Interni; Application, room: Esterno, ingressi di abitazioni, perimetro della casa, terrazzi / balconi, Cortili e passi carrai; Colour: antracite; Colour, RAL: 7016; Includes corner wall mount: No; Installation site: Parete, angolo; Installation: In superficie, Parete, angolo; IP-rating: IP54; Ambient temperature: da -20 fino a 50 °C; Materiale: Plastica; Mains power supply: 230 V / 50 Hz; Switching output 1, resistive: 1000 W; Switching output 1, floating: No; Fluorescent lamps, electronic ballast: 1000 W; Fluorescent lamps, uncorrected: 500 VA; Fluorescent lamps, series-corrected: 900 VA; Fluorescent lamps, parallel-corrected: 500 VA; Switching output 1, low-voltage halogen lamps: 1000 VA; LED lamps < 2 W: 100 W; LED lamps > 2 W < 8 W: 175 W; LED lamps > 8 W: 350 W; Capacitive load in μF: 132 µF; Power consumption: 0,5 W; Technology, sensors: Infrarossi passivi, Sensore ottico; Mounting height: 1,8 – 4 m; Mounting height max.: 4,00 m; Optimum mounting height: 2 m; Detection angle: 180 °; Angle of aperture: 90 °; Sneak-by guard: Sì; Capability of masking out individual segments: Sì; Electronic scalability: No; Mechanical scalability: No; Reach, radial: r = 1.5 m (4 m²) / r = 3 m (14 m²); Reach, tangential: r = 5 m (39 m²) / r = 12 m (226 m²); Switching zones: 508 zone di commutazione; Cover material: calotte di copertura; Twilight setting: 2 – 2000 lx; Time setting: 5 sec – 15 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Sì; Type of interconnection: master/master; Interconnection via: Cavo; Product category: Sensore di movimento

**Produttore** Steinel

**Art. n.** 057664

**Denominazione ordine** IS 2180-2 antracite

Consegnare, montare e impostare in modo che sia pronto alla messa in funzione