**STEINEL Professional Motion detector**

**IS 2360 DE ECO 8m**

**white**

Dimensions (Ø x H): 78 x 89 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Potentiometers; With remote control: No; Version: white; PU1, EAN: 4007841034733; Type: Motion detectors; Application, place: Outdoors, Indoors; Application, room: corridor / aisle, changing room, function room / ancillary room, kitchenette, stairwell, WC / washroom, outdoors, front door, all round the building, terrace / balcony, Indoors; Colour: white; Colour, RAL: 9010; Includes corner wall mount: No; Installation site: ceiling; Installation: In-ceiling installation, Ceiling; IP-rating: IP54; Protection class: II; Ambient temperature: -20 – 40 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, number of LEDs / fluorescent lamps: 6 pcs.; Fluorescent lamps, electronic ballast: 430 W; Fluorescent lamps, uncorrected: 500 VA; Fluorescent lamps, series-corrected: 406 VA; Fluorescent lamps, parallel-corrected: 406 VA; Switching output 1, low-voltage halogen lamps: 1000 VA; LED lamps < 2 W: 16 W; LED lamps > 2 W < 8 W: 64 W; LED lamps > 8 W: 64 W; Capacitive load in μF: 132 µF; Technology, sensors: passive infrared, Light sensor; Mounting height: 2,2 – 4 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,5 m; Detection angle: 360 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: No; Reach, radial: Ø 4 m (13 m²); Reach, tangential: Ø 8 m (50 m²); Cover material: shrouds; Twilight setting: 2 – 2000 lx; Time setting: 8 sec – 35 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/master; Interconnection via: Cable

**Manufacturer** Steinel

**Prod. No.** 034733

**Ordering designation** IS 2360 DE ECO 8m white

Deliver, install and set ready for operation