**STEINEL Professional Motion detector**

**IS 2360 ECO 7m**

**white**

Dimensions (Ø x H): 115 x 51 mm; Manufacturer's Warranty: 5 years; Settings via: Potentiometers; With remote control: No; Version: white; PU1, EAN: 4007841006556; Type: Motion detectors; Application, place: Outdoors, Indoors; Application, room: corridor / aisle, changing room, function room / ancillary room, kitchenette, stairwell, WC / washroom, multi-storey / underground car park, outdoors, warehouse, Indoors; Colour: white; Colour, RAL: 9010; Includes corner wall mount: No; Installation site: ceiling; Installation: Surface wiring, Ceiling; IP-rating: IP54; Ambient temperature: from -20 up to 50 °C; Material: Plastic; Mains power supply: 230 V / 50 – 60 Hz; Switching output 1, resistive: 2000 W; Switching output 1, number of LEDs / fluorescent lamps: 50 pcs.; Fluorescent lamps, electronic ballast: 350 W; Fluorescent lamps, uncorrected: 500 VA; Fluorescent lamps, series-corrected: 500 VA; Fluorescent lamps, parallel-corrected: 500 VA; Switching output 1, low-voltage halogen lamps: 1000 VA; LED lamps < 2 W: 100 W; LED lamps > 2 W < 8 W: 175 W; LED lamps > 8 W: 350 W; Capacitive load in μF: 132 µF; Technology, sensors: passive infrared, Light sensor; Mounting height: 2,00 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: No; Reach, radial: Ø 3 m (7 m²); Reach, tangential: Ø 7 m (38 m²); Switching zones: 664 switching zones; Twilight setting: 2 – 2000 lx; Time setting: 8 sec – 35 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/master; Interconnection via: Cable; Interconnection, number: max 5 sensors; Product category: Motion detector

**Manufacturer** Steinel

**Prod. No.** 006556

**Ordering designation** IS 2360 ECO 7m white

Deliver, install and set ready for operation