STEINEL Professional Motion detector

IS 2360-3 ECO 24m
white

Dimensions (Ø x H): 121 x 57 mm;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: Potentiometers;With remote control: No;Version: white;PU1, EAN: 4007841057770;Type: Motion detectors;Application, place: Outdoors, Indoors;Application, room: corridor / aisle, changing room, function room / ancillary room, kitchenette, stairwell, WC / washroom, multi-storey / underground car park, outdoors, warehouse, Indoors;Colour: white;Colour, RAL: 9010;Includes corner wall mount: No;Installation site: ceiling;Package content: 1;Installation: Surface wiring, Ceiling;IP-rating: IP54;Protection class: II;Ambient temperature: from -20 up to 50 °C;Material: Plastic;Mains power supply: 220 – 240 V / 50 – 60 Hz;Switching output 1, resistive: 2000 W;Switching output 1, number of LEDs / fluorescent lamps: 8 pcs.;Switching output 1, floating: No;Fluorescent lamps, electronic ballast: 500 W;Fluorescent lamps, uncorrected: 500 VA;Fluorescent lamps, series-corrected: 900 VA;Fluorescent lamps, parallel-corrected: 400 VA;Switching output 1, low-voltage halogen lamps: 2000 VA;LED lamps < 2 W: 100 W;LED lamps > 2 W < 8 W: 300 W;LED lamps > 8 W: 500 W;Capacitive load in μF: 176 µF;Power consumption: 0,56 W;Technology, sensors: passive infrared, Mixed light metering;Voltage range (min): 220 V;Voltage range (max): 240 V;Mounting height: 2,50 – 6,00 m;Mounting height max.: 6,00 m;Optimum mounting height: 2,8 m;Detection angle: 360 °;Angle of aperture: 90 °;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: No;Mechanical scalability: No;Reach, radial: Ø 6 m (28 m²);Reach, tangential: Ø 24 m (452 m²);Switching zones: 972 switching zones;Cover material: shrouds;Twilight setting: 2 – 1000 lx;Time setting: 5 sec – 15 min;Basic light level function: No;Main light adjustable: No;Twilight setting TEACH: No;Constant-lighting control: No;Interconnection: Yes;Type of interconnection: Master/master;Interconnection via: Cable;Interconnection, number: max 5 sensors;Product category: Motion detector

Manufacturer Steinel
Prod. No. 057770
Ordering designation IS 2360-3 ECO 24m white

Deliver, install and set ready for operation
