STEINEL Professional Motion detector

sensIQ S
Anthracite EVO

Dimensions (L x W x H): 128 x 114 x 74 mm;With motion detector: Yes;Manufacturer's Warranty: 5 years;Settings via: Remote control, Potentiometers, Smart Remote;With remote control: Yes;Version: Anthracite;PU1, EAN: 4007841056650;Type: Motion detectors;Application, place: Indoors, Outdoors;Application, room: multi-storey / underground car park, outdoors, warehouse, front door, all round the building, courtyard & driveway, Indoors;Colour: Anthracite;Colour, RAL: 7016;Includes corner wall mount: Yes;Installation site: wall, corner;Installation: Surface wiring, Wall, corner;IP-rating: IP54;Ambient temperature: from -20 up to 50 °C;Material: Plastic;Mains power supply: 100 – 240 V / 50 – 60 Hz;Switching output 1, resistive: 2000 W;Switching output 1, number of LEDs / fluorescent lamps: 50 pcs.;Fluorescent lamps, electronic ballast: 1500 W;Fluorescent lamps, uncorrected: 1000 VA;Fluorescent lamps, series-corrected: 700 VA;Fluorescent lamps, parallel-corrected: 1000 VA;Switching output 1, low-voltage halogen lamps: 1000 VA;LED lamps < 2 W: 100 W;LED lamps > 2 W < 8 W: 300 W;LED lamps > 8 W: 600 W;Capacitive load in μF: 176 µF;Power supply, detail: 500 VA max., 120 V;Technology, sensors: passive infrared, Mixed light metering;Voltage range (min): 100 V;Voltage range (max): 240 V;Mounting height: 2,00 – 5,00 m;Mounting height max.: 5,00 m;Optimum mounting height: 2 m;Detection angle: 300 °;Angle of aperture: 180 °;Sneak-by guard: Yes;Capability of masking out individual segments: Yes;Electronic scalability: No;Mechanical scalability: Yes;Reach, radial: r = 4 m (42 m²);Reach, tangential: r = 20 m (1047 m²);Switching zones: 1360 switching zones;Functions: Normal / test mode, Manual ON / ON-OFF;Twilight setting: 2 – 1000 lx;Time setting: 5 sec – 15 min;Basic light level function: No;Main light adjustable: No;Twilight setting TEACH: Yes;Constant-lighting control: No;Interconnection: Yes;Type of interconnection: Master/master;Interconnection via: Cable;Product category: Motion detector

Manufacturer Steinel
Prod. No. 056650
Ordering designation sensIQ S Anthracite

Deliver, install and set ready for operation
