**STEINEL Professional Motion detector**

**sensIQ S**

**white EVO**

Dimensions (L x W x H): 128 x 114 x 74 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Remote control, Potentiometers, Smart Remote; With remote control: Yes; Version: white; PU1, EAN: 4007841034955; Type: Other; Application, place: Indoors, Outdoors; Application, room: multi-storey / underground car park, outdoors, warehouse, front door, all round the building, courtyard & driveway, Indoors; Colour: white; Colour, RAL: 9010; Includes corner wall mount: Yes; Installation site: wall, corner; Installation: Surface wiring, Wall, corner; IP-rating: IP54; Ambient temperature: from -20 up to 50 °C; Material: Plastic; Mains power supply: 100 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 2000 W; Switching output 1, number of LEDs / fluorescent lamps: 50 pcs.; Fluorescent lamps, electronic ballast: 1500 W; Fluorescent lamps, uncorrected: 1000 VA; Fluorescent lamps, series-corrected: 700 VA; Fluorescent lamps, parallel-corrected: 1000 VA; Switching output 1, low-voltage halogen lamps: 1000 VA; LED lamps < 2 W: 100 W; LED lamps > 2 W < 8 W: 300 W; LED lamps > 8 W: 600 W; Capacitive load in μF: 176 µF; Power supply, detail: 500 VA max., 120 V; Technology, sensors: passive infrared, Light sensor; Mounting height: 2,00 – 5,00 m; Mounting height max.: 5,00 m; Optimum mounting height: 2 m; Detection angle: 300 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: Yes; Reach, radial: r = 4 m (42 m²); Reach, tangential: r = 20 m (1047 m²); Switching zones: 1360 switching zones; Functions: Normal / test mode, Manual ON / ON-OFF; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: Yes; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/master; Interconnection via: Cable; Product category: Motion detector

**Manufacturer** Steinel

**Prod. No.** 034955

**Ordering designation** sensIQ S white

Deliver, install and set ready for operation