**STEINEL Professional Photoelectric lighting controller**

**Light Sensor Dual**

**DALI-2 Input Device - concealed, rd.**

Dimensions (Ø x H): 124 x 51 mm; With motion detector: No; Manufacturer's Warranty: 5 years; Settings via: Bus; Version: DALI-2 Input Device - concealed, rd.; PU1, EAN: 4007841057442; Type: Constant-lighting controller; Application, place: Outdoors, Indoors; Application, room: classroom, one-person office, open-plan office, high-bay warehouse, conference room / meeting room, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: wall, ceiling; Installation: Concealed wiring, Wall, Ceiling; IP-rating: IP20; Ambient temperature: from -20 up to 50 °C; Material: Plastic; Mains power supply: 12 – 22,5 V; Power supply, detail: DALI bus; Steuerausgang, Dali: Addressable/slave; Technology, sensors: Light sensor; Mounting height: 2,00 – 4,00 m; Mounting height max.: 4,00 m; Twilight setting: 2 – 1000 lx; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: No; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: DALI bus; Product category: Photoelectric lighting controller

**Manufacturer** Steinel

**Prod. No.** 057442

**Ordering designation** Light Sensor Dual DALI-2 Input Device - concealed, rd.

Deliver, install and set ready for operation