**STEINEL Professional Presence detector**

**IR Quattro MICRO 6m**

**DALI-2 Input Device - white**

Dimensions (Ø x H): 43 x 75 mm; With motion detector: Yes; Manufacturer's Warranty: 5 years; Settings via: Bus; With remote control: No; Version: DALI-2 Input Device - white; PU1, EAN: 4007841053871; Type: Presence detector; Application, place: Indoors; Application, room: one-person office, hotel room, care room, function room / ancillary room, WC / washroom, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: In-ceiling installation, Ceiling; IP-rating: IP65; Ambient temperature: -25 – 55 °C; Material: Plastic; Mains power supply: 12 – 22,5 V; Power supply, detail: DALI bus; Number of Dali users: 2; Steuerausgang, Dali: Addressable/slave; With bus coupling: Yes; Technology, sensors: passive infrared, Light sensor; Mounting height: 2,00 – 5,00 m; Mounting height max.: 5,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 90 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: No; Mechanical scalability: No; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 6 x 6 m (36 m²); Reach, presence: 4 x 4 m (16 m²); Switching zones: 168 switching zones; Twilight setting: 2 – 1000 lx; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: Yes; Constant-lighting control: Yes; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: DALI bus; Rated current: 4 mA; Max. Current consumption according to IEC 62386-101: 12 mA; Typical current consumption at 16V input voltage: 4 mA; Max. Current consumption at 10V input voltage in regular operation: 5 mA

**Manufacturer** Steinel

**Prod. No.** 053871

**Ordering designation** IR Quattro MICRO 6m DALI-2 Input Device - white

Deliver, install and set ready for operation