**STEINEL Professional Presence detector**

**IR Quattro SLIM XS 4m**

**COM1 - square**

Dimensions (L x W x H): 55 x 80 x 80 mm; Manufacturer's Warranty: 5 years; Settings via: Remote control, Smart Remote; With remote control: Yes; Version: COM1 - square; PU1, EAN: 4007841032951; Type: Presence detector; Application, place: Indoors; Application, room: one-person office, hotel room, care room, function room / ancillary room, WC / washroom, Indoors; Colour: white; Colour, RAL: 9010; Includes corner wall mount: No; Installation site: ceiling; Installation: In-ceiling installation, Ceiling; IP-rating: IP20; Ambient temperature: 0 – 40 °C; Material: Plastic; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 1000 W; Switching output 1, number of LEDs / fluorescent lamps: 8 pcs.; Fluorescent lamps, electronic ballast: 400 W; Fluorescent lamps, uncorrected: 500 VA; Fluorescent lamps, series-corrected: 500 VA; Fluorescent lamps, parallel-corrected: 500 VA; Switching output 1, low-voltage halogen lamps: 500 VA; LED lamps < 2 W: 16 W; LED lamps > 2 W < 8 W: 64 W; LED lamps > 8 W: 64 W; Capacitive load in μF: 176 µF; Technology, sensors: passive infrared, Light sensor; Mounting height: 2,50 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; Detection angle: 360 °; Angle of aperture: 71 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: No; Mechanical scalability: No; Reach, radial: 4 x 4 m (16 m²); Reach, tangential: 4 x 4 m (16 m²); Reach, presence: 4 x 4 m (16 m²); Switching zones: 408 switching zones; Functions: Normal / test mode, Semi-/fully automatic, Manual ON / ON-OFF; Twilight setting: 10 – 1000 lx; Time setting: 60 sec – 30 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: Yes; Constant-lighting control: No; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; Interconnection via: Cable

**Manufacturer** Steinel

**Prod. No.** 032951

**Ordering designation** IR Quattro SLIM XS 4m COM1 - square

Deliver, install and set ready for operation