**STEINEL Professional Rilevatore di presenza**

**True Presence**

**COM2 - sup. bianco**

Dimensions (L x W x H): 45 x 123 x 123 mm; With motion detector: Sì; Manufacturer's Warranty: 5 anni; Settings via: Bluetooth; With remote control: No; Version: COM2 - sup. bianco; PU1, EAN: 4007841057930; Type: Rilevatore di presenza; Application, place: Interni; Application, room: aula, auditorium, ufficio singolo, ufficio open space, magazzino verticale, aree di produzione, sala conferenze / sale riunioni, camere di hotel, camere assistite, camere di servizio, aree di soggiorno, sale pranzo / mense, spogliatoi, cucinette, palestra, reception / hall, WC / docce, magazzino, Interni; Colour: bianco; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: soffitto; Installation: In superficie, Soffitto; IP-rating: IP54; Ambient temperature: da -20 fino a 50 °C; Materiale: Plastica; Mains power supply: 220 – 240 V / 50 – 60 Hz; Switching output 1, resistive: 2000 W; Switching output 1, number of LEDs / fluorescent lamps: 8 pz; Switching output 1, floating: No; Switching output 2, resistive: 230 W; Switching output 2, floating: Sì; Fluorescent lamps, electronic ballast: 1500 W; Fluorescent lamps, uncorrected: 1000 VA; Fluorescent lamps, series-corrected: 400 VA; Fluorescent lamps, parallel-corrected: 1000 VA; Switching output 1, low-voltage halogen lamps: 2000 VA; LED lamps < 2 W: 100 W; LED lamps > 2 W < 8 W: 300 W; LED lamps > 8 W: 600 W; Capacitive load in μF: 176 µF; Power consumption: 1 W; Technology, sensors: Alta frequenza, Sensore ottico; Mounting height: 2,00 – 12,00 m; Mounting height max.: 12,00 m; Optimum mounting height: 2,8 m; Montagehöhe max. True Presence Erfassung: 4,00 m; HF-system: 7,2 GHz; Detection: anche attraverso vetro, legno e pareti in materiale leggero; Detection angle: 360 °; Angle of aperture: 160 °; Sneak-by guard: Sì; Capability of masking out individual segments: No; Electronic scalability: Sì; Mechanical scalability: No; Reach, radial: Ø 15 m (177 m²); Reach, tangential: Ø 15 m (177 m²); Reach, presence: Ø 15 m (177 m²); True Presence reach: Ø 9 m (64 m²); Transmitter power: < 1 mW; Functions: Parametrizzazione di gruppi, Modo semiautomatico/automatico, Scenario luminoso, Manuale ON / ON-OFF, Funzione di gruppo vicino, Modalità normale / modalità test; Twilight setting: 2 – 2000 lx; Time setting: 20 sec – 60 min; Basic light level function: No; Main light adjustable: No; Twilight setting TEACH: Sì; Constant-lighting control: No; Interconnection: Sì; Type of interconnection: master/master, Master/Slave; Interconnection via: Bluetooth; Product category: Rilevatore di presenza

**Produttore** Steinel

**Art. n.** 057930

**Denominazione ordine** True Presence COM2 - sup. bianco

Consegnare, montare e impostare in modo che sia pronto alla messa in funzione