**STEINEL Professional Motion detector**

**HF 3360**

**KNX - surface, sq. V3**

Dimensions (L x W x H): 52 x 95 x 95 mm; Manufacturer's Warranty: 5 years; Settings via: ETS software, Remote control, Bus, Smart Remote; With remote control: No; Version: KNX - surface, sq.; PU1, EAN: 4007841058210; Type: Motion detectors; Application, place: Indoors; Application, room: function room / ancillary room, stairwell, WC / washroom, multi-storey / underground car park, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: wall, ceiling, corner; Installation: Surface wiring, Wall, Ceiling, corner; IP-rating: IP54; Ambient temperature: -20 – 50 °C; Material: Plastic; Power supply, detail: KNX bus; With bus coupling: Yes; Technology, sensors: High frequency, Light sensor; Mounting height: 2,00 – 4,00 m; Mounting height max.: 4,00 m; Optimum mounting height: 2,8 m; HF-system: 5,8 GHz; Detection: also through glass, wood and stud walls; Detection angle: 360 °; Angle of aperture: 180 °; Sneak-by guard: Yes; Capability of masking out individual segments: No; Electronic scalability: Yes; Mechanical scalability: No; Reach, radial: Ø 8 m (50 m²); Reach, tangential: Ø 8 m (50 m²); Transmitter power: < 1 mW; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Basic light level function: Yes; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Yes; Constant-lighting control: Yes; KNX functions: Photo-cell controller, Basic light level function, Light level, HVAC output, Constant-lighting control, Light output 2x, Presence output, Day / night function, Logic gate; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: KNX bus; Rated current: 12,5 mA

**Manufacturer** Steinel

**Prod. No.** 058210

**Ordering designation** HF 3360 KNX - surface, sq.

Deliver, install and set ready for operation