**STEINEL Professional Motion detector**

**IS 345 MX Highbay**

**KNX - surface, sq. V3**

Dimensions (L x W x H): 65 x 95 x 95 mm; Manufacturer's Warranty: 5 years; Settings via: ETS software, Remote control, Bus, Smart Remote; With remote control: No; Version: KNX - surface, sq.; PU1, EAN: 4007841058296; Type: Motion detectors; Application, place: Indoors; Application, room: high-bay warehouse, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: ceiling; Installation: Surface wiring, Ceiling; IP-rating: IP54; Ambient temperature: from -20 up to 50 °C; Material: Plastic; Power supply, detail: KNX bus; With bus coupling: Yes; Technology, sensors: passive infrared, Light sensor; Mounting height: 4,00 – 16,00 m; Mounting height max.: 16,00 m; Optimum mounting height: 12 m; Detection angle: Aisle, 360 °; Angle of aperture: 90 °; Sneak-by guard: Yes; Capability of masking out individual segments: Yes; Electronic scalability: No; Mechanical scalability: No; Reach, radial: 30 x 4 m (120 m²); Reach, tangential: 30 x 4 m (120 m²); Switching zones: 280 switching zones; Twilight setting: 2 – 1000 lx; Time setting: 5 sec – 15 min; Basic light level function: Yes; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Yes; Constant-lighting control: Yes; KNX functions: Photo-cell controller, Basic light level function, Light level, HVAC output, Constant-lighting control, Light output 2x, Presence output, Day / night function, Logic gate; Interconnection: Yes; Type of interconnection: Master/slave; Interconnection via: KNX bus; Rated current: 12,5 mA; Product category: Motion detector

**Manufacturer** Steinel

**Prod. No.** 058296

**Ordering designation** IS 345 MX Highbay KNX - surface, sq.

Deliver, install and set ready for operation