**STEINEL Professional Photoelectric lighting controller**

**Light Sensor Dual**

**KNX - concealed, rd. V3**

Dimensions (Ø x H): 124 x 51 mm; Manufacturer's Warranty: 5 years; Settings via: ETS software, Remote control, Bus, Smart Remote; Version: KNX - concealed, rd.; PU1, EAN: 4007841058340; Type: Constant-lighting controller; Application, place: Outdoors, Indoors; Application, room: classroom, one-person office, open-plan office, high-bay warehouse, conference room / meeting room, Indoors; Colour: white; Colour, RAL: 9003; Includes corner wall mount: No; Installation site: wall, ceiling; Installation: Concealed wiring, Wall, Ceiling; IP-rating: IP20; Ambient temperature: -20 – 50 °C; Power supply, detail: KNX bus; With bus coupling: Yes; Mounting height: 2,00 – 4,00 m; Mounting height max.: 4,00 m; Twilight setting: 2 – 1000 lx; Basic light level function: Yes; Main light adjustable: 0 - 100 %; Twilight setting TEACH: Yes; Constant-lighting control: Yes; KNX functions: Light output 2x, Light level, Constant-lighting control, Photo-cell controller, Logic gate; Interconnection: Yes; Type of interconnection: Master/master, Master/slave; Interconnection via: KNX bus; Rated current: 12,5 mA

**Manufacturer** Steinel

**Prod. No.** 058340

**Ordering designation** Light Sensor Dual KNX - concealed, rd.

Deliver, install and set ready for operation