**STEINEL Professional Accessory**

**R-series emergency light module**

Dimensions (L x W x H): 20 x 66 x 101 mm; Manufacturer's Warranty: 5 years; With remote control: No; PU1, EAN: 4007841064143; Colour: white; Protection class: without; Ambient temperature: 0 – 40 °C; Housing material: Plastic; Mains power supply: 3,6 V; Power supply, detail: Batteries (included), 3 x batteries, type AAA; Interconnection: No; Luminous flux, emergency light: 107 lm

**Manufacturer** Steinel

**Prod. No.** 064143

**Ordering designation** R-series emergency light module

Deliver, install and set ready for operation