**STEINEL Professional System components**

PU1, EAN: 4007841089191; IP-rating: IP20; Protection class: II; Ambient temperature: -5 – 45 °C; With bus coupling: Yes

**Manufacturer** Steinel

**Prod. No.** 089191

**Ordering designation**

Deliver, install and set ready for operation