STEINEL DIY Outdoor light without sensor

L 15
white

Dimensions (L x W x H): 243 x 188 x 404 mm;With lamp: No;Manufacturer's Warranty: 3 years;With remote control: No;Version: white;PU1, EAN: 4007841069186;Application, place: Outdoors;Application, room: outdoors, front door, courtyard & driveway, terrace / balcony, all round the building;Colour: white;includes sheet of self-adhesive numbers: No;Package content: 1;Installation site: wall;Impact resistance: IK03;IP-rating: IP44;Protection class: II;Ambient temperature: from -20 up to 40 °C;Housing material: Plastic;Cover material: Plastic, transparent;Mains power supply: 230 – 240 V / 50 Hz;Output: 60 W;Mounting height max.: 3,00 m;Photo-cell controller: No;Lamp: All-purpose lamp;Base: E27;Basic light level function: No;Twilight setting TEACH: No;Interconnection: No;Optimum mounting height: 2 m;Product category: Outdoor light without sensor

Manufacturer Steinel
Prod. No. 069186
Ordering designation L 15 white

Deliver, install and set ready for operation
