STEINEL Professional System components

IPR500 KNX-S IP Router


Manufacturer's Warranty: 5 years;Settings via: Bus;PU1, EAN: 4007841095956;Application, place: Indoors;Colour: grey;Installation: Other;IP-rating: IP20;Protection class: III;Ambient temperature: from -5 up to 45 °C;Power supply, detail: KNX bus;With bus coupling: Yes;Functions: Configuration interface;KNX Medium: TP 256;KNX Secure: Yes;Product category: System components;KNX functions – technical details: KNXnet/IP routing, KNXnet/IP tunneling, 8 tunnel connections, Support of KNX Security, Support of KNX Long Frames, Extended filter table for main group 0..31, Buffer for 150 telegrams, Status display via 3 LEDs, Power supply via KNX bus, Connections: KNX, LAN RJ-45, For DIN rail, width 1 unit (18 mm);Stromaufnahme Bus Eingabe: 20 mA

Manufacturer Steinel
Prod. No. 095956
Ordering designation IPR500 KNX-S IP Router

Deliver, install and set ready for operation
